COS Above Ceiling Punchlist 6 2nd Floor

OK to drop ceiling tile in the following rooms:

202,203. 204,205, 216, 214, 216A

Room 216A

1. Install register and slack wire.

Room 202

1. Add extension to electrical junction box.

Room 215B

1. Duct strapping at plenum and ductwork needs to be added. Please have David contact to review.
2. Install proper length screws at wall angle (located in small room)
3. Install splay wire; see masking tape.